Namrup

Annexure-I

Ref.: N-III/Mech-5/Cont-992

**Job list:**

|  |  |  |  |
| --- | --- | --- | --- |
| Sl. No. | Item | Unit | Quantity |
| 1.0 | Waste heat recovery section manhole cover | | |
| 1.1 | waste heat recovery section manhole cover opening and Boxed up (Ø14”), 03nos | ID | 14”x3= 42 |
| 2.0 | Auxiliary fire Superheater manhole cover & Start up heater manhole cover | | |
| 2.1 | Auxiliary fire Superheater & Start up heater manhole cover opening and Boxed up (Ø14”), 02nos | ID | 14”x2=28 |
| 3.0 | Primary reformer manhole cover opening and boxed up job | | |
| 3.1 | Primary reformer manhole cover 04 nos opening & boxed up job(Ø30”) | ID | 30”x4=120 |
| 4.0 | RG boiler bottom hand hole cover flange opening and boxed up job | | |
| 4.1 | RG boiler bottom hand hole cover flange opening and boxed up job (Ø2”), 01 no. | ID | 2”x1=2 |

**General SCOPE OF WORK**

Scope of work shall include but not limited to the following:

1. Cutting of all necessary gaskets in proper dimensions from supplied gasket sheets.
2. Proper cleaning of gasket jointing surface
3. Fitting of supplied gaskets properly without damage.
4. Appropriate tightening of all nuts-bolts.
5. All the tools & tackles and accessories shall be adequately supplied by the executing agency.
6. All best engineering practices & procedures and safety gadgets to be strictly followed while working.
7. Carrying/cleaning of site debris/waste to dumping yard after finishing of job.
8. Returning of unused supplied material(s) to the Engineer-in-charge.
9. Job shall be executed as instructed by Engineer-in-charge

(PK Barkataki)

PE (M), A-III

**Annexure-II**

**Ref**: N-III/MECH-5/Cont-992

**SCHEDULE OF WORK & QUANTITY:**

iv) Present market rate.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Sl. No. | Item | Unit | Quantity | Unit Rate (**`**) | Amount (**`**) |
| 2.0 | Waste heat recovery section manhole cover opening and Boxed up | ID | 42 |  |  |
| 3.0 | Auxiliary fire Superheater cover & Start up heater manhole cover opening and Boxed up | ID | 28 |  |  |
| 4.0 | Primary reformer manhole cover | ID | 120 |  |  |
| 5.0 | RG boiler bottom hand hole cover | ID | 2 |  |  |
| Sub total | | | | |  |
| G.S.T. @ 18% | | | | |  |
| Total | | | | |  |

**NOTE:** Party to fill the tender form with clear handwriting as instructed and avoid overwriting.

1. Party to write “**Not Registered ”,** if the **GST** is applicable.
2. Party to fill the tender form with clear handwriting as instructed and avoid overwriting.

In words: (Rupees ……………………………………………………………………………………………………………………………

………………………………………………………………………………………………………………………………………………….. only

----------------------------------------------------------------------------------------------------------

Signature of the tenderer with Date:

Party’s name:

Address:

SEAL: PAN No.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**……………………………………………………………………………………………………………………**