Ref: N-III/18/Mech-CPP/Cont-669/

**Tender Document**

1.00 Name of work: Execution of various insulation & refractory jobs on Service Boiler and waste heat boiler in CPP

Job Details:

1. Repairing of insulation work of Side wall of secondary super heater zone of Service Boiler.
2. Repairing of insulation work of both manhole cover portion and bottom end of Mud drum.
3. Repairing of damaged refractory works of furnace zone of WHB-II
4. Fabrication of Aluminum sheet between flex seal in exhaust plenum aft wall
5. Repairing of damaged refractory wall of furnace zone of service boiler
6. Repairing of air conditioning duct for control room of CPP.

2.00 Terms & conditions:

2.01 The Tenderer(s) may visit the site to assess quantum & nature of job.

2.02 Required man Power for execution of job shall be arranged by the party.

2.03 All required tools & tackles shall be arranged by the party.

2.04 Scaffolding if required will be in the scope of the party.

2.05 All necessary safety precautions are to be taken by the party.

* 1. SPECIAL TERMS & CONDITIONS

3.01 The contractors have to abide by the terms and conditions mentioned in G.D.C.C. in respect of Carrying out the job, payments, settlement of disputes etc.

* 1. All works are to be done under the strict supervision of the contractor to the entire satisfaction of the Engineer-in-charge / site in charge.

3.03 All Safety measure and gears required for the job shall have to be arranged by the contractor and to be followed strictly.

3.04 After completion of job, the site shall be cleaned and removed all debris properly.

4.00 EARNEST MONEY: The tenderers shall deposit the Earnest money in the form of an A/c. Payee Demand Draft, payable at SBI, Namrup (Branch Code: 0223.) drawn in favour of M/s. Brahmaputra Valley Fertilizers Corporation Limited, Namrup. No interest shall be payable on EMD. The tender (s) without earnest money shall be rejected.

NSIC/MSME registered companies shall produce valid copy of registration certificate for exemption of EMD.

5.00 Payment Terms

5.01 90% payment shall be made after completion of job. Balance 10% payment shall be kept as Security Deposit (SD), which shall be release after successful completion of workmanship guarantee period of 06(six) month.

5.02 Balance 10% shall be retained as Security Deposit unless a Bank guarantee from a scheduled bank is executed in lieu of that for the equivalent sum. SD will be released after expiry of workmanship guarantee period of 6(six) months to be valid from the date of completion of the jobs.

6.00 Party shall quote & submit their rates in the given pro-forma in Annexure-II by going thoroughly in the scope of work at Annexure-I.

7.00 The contractor shall abide by all the statutory obligation under various statutory Acts and rules made there under, and as amended from time to time in respect of their establishment and / or workmen engaged by them. Under any circumstances, BVFCL shall not be liable or held responsible in any manner whatsoever, for default or omission on the part of the contractor(s) for non-compliance of the aforesaid Acts and rules, and any other laws applicable to contractors and / or their establishment and the workmen engaged by them.

8.00 BVFCL is committed to a corruption free environment.” All the works contract, services and commitments of BVFCL will be honored without the citizen having to pay any bribe”. In case any person demands any bribe, it is the duty of responsible citizen to inform the matter to Vigilance Office, BVFCL, Namrup, Assam. (Tel No: 0374 2507092/ 0374 2507167).

(M.Hoque)

PE (M), CPP&CMW

Annexure-I

Ref: N-III/18/Mech-CPP/Cont-669/

**Scope of work**

Name of work : Execution of various insulation & refractory jobs on Service Boiler and waste

heat boiler in CPP

JOB Details:

1. Repairing of insulation work of Side wall of secondary super heater zone of Service Boiler.
2. Repairing of insulation work of both manhole cover portion and bottom end of Mud drum.
3. Repairing of damaged refractory works of furnace zone of WHB-II
4. Fabrication of Aluminum sheet between flex seal in exhaust plenum aft wall
5. Repairing of damaged refractory wall of furnace zone of service boiler
6. Repairing of air conditioning duct for control room of CPP.

Material Required:

1. New Aluminum Sheet of Grade: 22 SWG (Qnty: 10 sqm2)
2. fixing screws, G.I. wires, aluminum strips, sealing compounds etc
3. Insulation material, refractory material will be supplied free of cost.

Scope of work shall include but shall not be limited to the following:

* 1. Shifting of insulation material (mineral wool) pads of 50 mm, refractory material (insulation brick, tabcast etc) from BVFCL Store to site
  2. Making of scaffoldings for working and accessing the job as and where required.
  3. Applying & fixing of new insulation material pads of 50 mm thickness.
  4. Covering the insulation by proper fixing of old aluminium sheets with screws.

1. Dismantling of scaffoldings, cleaning of site debris/ waste to dumping yard after completion of job.
2. Returning of unused supplied materials to the site store.

**Note:**-

1. Arrangement of all tools & tackles required for entire job shall be in party’s scope.
2. All the lifting, hosting & grounding arrangement like hoist, chain pulley blocks etc. required for the entire scope of work shall be arranged by the party at their own cost.
3. New aluminum sheets if required, fixing screws, G.I. wires, aluminium strips, sealing compounds etc. shall be arranged by the party at their own cost.
4. Proper scaffolding, if and wherever required for safe execution of the work shall be under party’s scope.
5. All standard engineering practices and safety procedures shall be followed till completion of the job.
6. The entire job shall be completed within 8 days.
7. Any other activities, not included above required for successful completion of the job shall be in the party’s scope.

(M. Hoque)

PE (M), CPP & CMW

ANNEXURE-II

**Ref. No**: N-III/18/MECH-CPP/CONT-669/

**PRO-FORMA FOR SCHEDULE OF WORK & QUANTITY**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl.No** | **Description of work:** | **Quantity** | Rate (`) | **(A)**  **Total amount (`)** |
| 1 | Execution of various insulation & refractory jobs on Service Boiler and waste heat boiler as per scope of work at annexure-I | 01(one) LOT |  |  |
| CGST @ 9% | | | |  |
| CGST @ 9% | | | |  |
| TOTAL | | | |  |

**NOTE:**

1. Party not to add GST if they are exempted and to write “**NOT APPLICABLE”,** but to attach proof copy issued from the competent/ statutory authority.
2. Party to add **GST,** if applicable.
3. Party to fill the tender form with clear handwriting as instructed and avoid overwriting.

In words: Rupees\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Only.

Signature of the Tenderer\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Party’s name:

Address:

SEAL: PAN No.\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**……………………………………………………………………………………………………………………**